# Parameter Area

The right side of the parameter editor window held the parameters of the chosen group

The following colums can be displayed. Which column is displayed can be set in the menu

### ParaID

The unique identification number of the parameter. if the parameter contains sub-ids the values can be displayed with a double-click on the parameter id.

### Name / Description

The name and the description of the parameter.

### Value

Actual value of the parameter. this value is read from the device in a regular cycle. The update frequency is normally 2 Hz but some cases, especially with high processor load or very slow network connections the update frequency can be much slower.

If a parameter is read only a lock symbol is shown on the left side of the parameter value.

Yellow lock: This parameter can not be written

Green lock: The writing can be temporarily enabled via "View" -> "Write Enable Protected Parameters“

### Data Type

the data type of the parameter.

# Layout of the Tabulators

With the double click on the parameter group a new tabulator group is opening in front of the already opened groups. All tabs can be moved with the mouse to a different position. Press with the left mouse button on the tab and hold it down. Move the mouse to another position. You can snap in the tab into any side of the window, or get a separate window for this tab.

(see example here)

# Context Menu

With a right click on any parameter a context sensitive menu opens with the following menu items:

### Graph

A new graph-window is opened or the actual parameter is added to an already existent graph window.

### Set Value

The parameter value is set to the minimum, maximum or default value.